G30 METAL PROFILED SHEET DECKING

**300 FIXINGS TO THE UNDERSIDE OF COMPOSITE FLOOR/SLAB**

**Specification:** Proprietary wedge nut fixings are available to suit differing profile geometries with a safe working load of 1kN per fixing.

Manufacturer: Lindapter International

 Lindsay House, Brackenbeck Road, Bradford, West Yorkshire, UK BD7 2NF

 Website: [www.lindapter.com](http://www.lindapter.com) Telephone: +44 (0)1274 521 444

Installation: To avoid possible localised overloading of the slab, fixings should not be locally grouped. As a guide nominal 600mm grid spacing is recommended as a minimum. Refer to manufacturer’s guidance for installation.



**‘V’ Nut wedge to suit R51 re-entrant profile**



**TR60 wedge to suit TR+ profiles (suitable for both TR60+ and TR80+)**